87     TL717
 
  BH • 00-SF  REA semi-curved  B  +  V- 8   LH
 
--------------------------------------------------------------
 
     Information  about  this  template :
 
( all dimensions in millimetres )
 
template generated at 11:34:06 on 08/07/2015 using Templot v:2.11.b
scale = 4.0 mm/ft     scale ratio = 1:76.2
track gauge = 16.2    flangeway gap = 1.0
template: straight
rail head only (bullhead): rails vertical
------------
LH turnout:
REA semi-curved  B-size left-hand switch (unjoggled)
1 in 8.00 RAM  ( 1 in 8.03 CLM ) regular V-crossing
square-on timbering
------------
adjacent track centres main side = 60.0
adjacent track centres turnout side = 120.0
angle at TXP crossover mid-point (CTRL-5) = 7.13 degrees ( 1 in 8.0 RAM )
angle at TVJP turnout road vee joint (CTRL-6) = 7.13 degrees ( 1 in 8.0 RAM )
------------
overall length = 300.83
approach/exit track in  60 ft rails / 25 sleepers per length ( rail length = 240.0 ):
approach track length = 0
exit track length = 0.52  ( 0 full rail lengths + 0 sleepers in 0.22 % of a rail length )
 
turnout-road centre-line radius (at turnout-curve) = 1731.34
 
switch-curve radius (rail gauge-face) = 2452.0
turnout-curve radius (rail gauge-face) = 1739.44
switch-curve radial centre: X = [ -25.6 ]  Y = 2443.62  (from CTRL-0)
turnout-curve radial centre: X = 13.03  Y = 1732.11  (from CTRL-0)
V-crossing entry-straight (curve-end to fine-point) = 16.0
 
switch front (rail-joint to switch-toe) = 21.67
virtual lead (switch-toe to fine-point) = 223.11
actual lead (switch-toe to blunt nose) = 225.13
blunt nose to timber A = [ -0.65 ]
width of blunt nose = 0.25
 
wing rail reach length (main-side) = 16.0
wing rail reach length (turnout-side) = 16.0
check rail overall length (main-side) = 52.0
check rail overall length (turnout-side) = 52.0
------------
smallest radius on this template = 1731 mm ( 68.2 " )
total angular swing on this template = 0 degrees (in main road)
------------
nominal gauge :   00-SF    16.2  mm    4 mm/ft     1:76.2    00 Special Fine EM dims
------------
template location on trackpad :
 
rotation :  X = 0   Y = 24.0   K = 0 degrees
  shift :  X = 1828.72   Y = 2143.02
rail-end :  X = 1828.72   Y = 2167.02
 
peg from origin :  X = 1828.72   Y = 2175.12   K = 0 degrees
peg from notch :  X = [ -40.2 ]   Y = 349.28   K = [ -340.86 ] degrees ( 1 in 2.88 RAM )

track centre-line radius at peg = straight  ( 3936811.02 " )
internal geometrical radius = 2089.77  ( 82.27 " )
external geometrical radius (substitution radius) = 2981.93  ( 117.4 " )
------------
 
total timbering length on this template = 1340.0
 
--------------------------------------------------------------
 
     Your  memo  notes  for  this  template :
 
your memo notes for this template ...

____________
v: 2.11.b   ©

   88     TL718
 
  BH • 00-SF  REA semi-curved  B  +  V- 8   LH
 
--------------------------------------------------------------
 
     Information  about  this  template :
 
( all dimensions in millimetres )
 
template generated at 11:36:25 on 08/07/2015 using Templot v:2.11.b
scale = 4.0 mm/ft     scale ratio = 1:76.2
track gauge = 16.2    flangeway gap = 1.0
template: straight
rail head only (bullhead): rails vertical
------------
LH turnout:
REA semi-curved  B-size left-hand switch (unjoggled)
1 in 8.00 RAM  ( 1 in 8.03 CLM ) regular V-crossing
square-on timbering
------------
adjacent track centres main side = 44.67
adjacent track centres turnout side = 44.67
angle at TXP crossover mid-point (CTRL-5) = 7.13 degrees ( 1 in 8.0 RAM )
angle at TVJP turnout road vee joint (CTRL-6) = 7.13 degrees ( 1 in 8.0 RAM )
------------
overall length = 293.41
approach/exit track in  60 ft rails / 25 sleepers per length ( rail length = 240.0 ):
approach track length = 0
exit track length = 0
 
turnout-road centre-line radius (at turnout-curve) = 1731.34
 
switch-curve radius (rail gauge-face) = 2452.0
turnout-curve radius (rail gauge-face) = 1739.44
switch-curve radial centre: X = [ -25.6 ]  Y = 2443.62  (from CTRL-0)
turnout-curve radial centre: X = 13.03  Y = 1732.11  (from CTRL-0)
V-crossing entry-straight (curve-end to fine-point) = 16.0
 
switch front (rail-joint to switch-toe) = 21.67
virtual lead (switch-toe to fine-point) = 223.11
actual lead (switch-toe to blunt nose) = 225.13
blunt nose to timber A = 1.33
width of blunt nose = 0.25
 
wing rail reach length (main-side) = 16.0
wing rail reach length (turnout-side) = 16.0
check rail overall length (main-side) = 52.0
check rail overall length (turnout-side) = 52.0
------------
smallest radius on this template = 1731 mm ( 68.2 " )
total angular swing on this template = 0 degrees (in main road)
------------
nominal gauge :   00-SF    16.2  mm    4 mm/ft     1:76.2    00 Special Fine EM dims
------------
template location on trackpad :
 
rotation :  X = 0   Y = 24.0   K = 0 degrees
  shift :  X = 1828.74   Y = 2089.73
rail-end :  X = 1828.74   Y = 2113.73
 
peg from origin :  X = 1828.74   Y = 2121.83   K = 0 degrees
peg from notch :  X = [ -40.18 ]   Y = 295.99   K = [ -340.86 ] degrees ( 1 in 2.88 RAM )

track centre-line radius at peg = straight  ( 3936811.02 " )
internal geometrical radius = 2089.77  ( 82.27 " )
external geometrical radius (substitution radius) = 3013.79  ( 118.65 " )
------------
 
total timbering length on this template = 1238.0
 
--------------------------------------------------------------
 
     Your  memo  notes  for  this  template :
 
your memo notes for this template ...

____________
v: 2.11.b   ©